Orbital inclination [deg].
97.769633124642752
Ascending (northwards) solar equator crossing time [h].
23.5
Date.
2015 1 1
Flag for providing revolution time or altitude. 0=revoluation time. 1=altitude.
0
Time of one revolution [h] or satellite altitude [km]. See previous flag.
1.6097560975609757
Longitude at daytime equator pass [deg].
0.0
Starting orbit phase, 0=night, 0.25=closest to first pole, 0.5=day equator, 0.75=closest to second pole, 1=night again.
0.25
Ending orbit phase, 0=night, 0.25=closest to first pole, 0.5=day equator, 0.75=closest to second pole, 1=night again.
0.50
Sampling time [s].
0.286
Number of detector rows.
170
Alpha angle polynomial values [deg], input number ranges from -1 (first row) to 1 (last row). Lowest order (zeroth) first.
0.0 -16.05
Beta angle polynomial values [deg], input number ranges from -1 (first row) to 1 (last row). Lowest order (zeroth) first.
0.0
